[RDXA] W1AW/2 Bands and modes

[Paul Mackanos - K2DB](https://us-mg5.mail.yahoo.com/neo/launch?.rand=42t3inu65t6mf)

Jan 29 at 9:47 AM

To rdxa@rdxa.com

RVHFG\_General@yahoogroups.com

wnydxa@yahoogroups.com

When we roll out the sign up calendar, these are the accepted bands and modes for W1AW/2 starting May 21st.I have yellow highlighted some stuff, and it should answer many questions. Vic, Carey and I have been “tweaking a sign – up calendar” and will roll it out when completed. At present, we are looking at 2 hour slots for operating.

Paul K2DB

Bands & Modes

To count for points, all QSOs must be two-way (no cross-band or cross-mode), using any of the modes CW, Phone (FM, SSB, AM, digital voice), or Digital (any digital mode, i.e. PSK31, RTTY). You are encouraged to work stations on each mode, but you may not work someone on three modes on the same frequency.  QSOs must be made within the following bands (some bands show suggested frequencies for modes that are not allowed in the USA -- stations outside the USA may use these frequencies if they desire for the QSO Party):

|  |  |  |  |
| --- | --- | --- | --- |
| Meters | CW | Phone | Digital |
| 160 | 1.800 – 1.843 | 1.843 – 1.900 | 1.800 -  1.843 |
| 80 | 3.500 – 3.600 | 3.600 – 4.000 | 3.525 – 3.600 |
| 40 | 7.000 – 7.125 | 7.040 – 7.300 | 7.025 – 7.100 |
| 30 | 10.100 – 10.150 |  | 10.110 – 10.150 |
| 20 | 14.000 – 14.150 | 14.110 – 14.350 | 14.025 – 14.150 |
| 17 | 18.068 – 18.110 | 18.110 – 18.168 | 18.090 – 18.110 |
| 15 | 21.000 – 21.200 | 21.110 – 21.450 | 21.025 – 21.200 |
| 12 | 24.890 - 24.930 | 24.930 – 24.990 | 24.900 – 24.930 |
| 10 | 28.000 – 28.300 | 28.200 – 29.700 | 28.025 – 28.200 |
| 6 | 50.000 – 50.125 | 50.100 – 50.500 | Use normally accepted frequencies |
| 2 | 144.010 – 144.200 | 144.100 – 148.000 | Use normally accepted frequencies |
| 1.25 | 222.000 – 225.000 | 222.000 – 225.000 | 222.000 – 225.000 |
| 70cm | 420.000 – 450.000 | 420.000 – 450.000 | 420.000 – 450.000 |
| 903 MHz & higher | | One QSO per band, per eligible station  is allowed regardless of mode | | |
| Satellites | | One QSO on any satellite per eligible station, regardless of mode, is allowed. | | | |
|  |  |  |  |  |  |